Sample number: 05PPT02	Site: (compass measurements includes correct inclination)	
Collector name: Darryl and Marc	Date: 09/July/05	
Before Collection: 		
Comments on sample in situ: On bench ~ 2m N of PPT01. Bedrock, sub planer surface with ~ 5mm roughness. Sample from slight concavity.

Dip/dip direction: Horizontal  10° dip direction E	
Lithology: Quartzite conglomerate	
Latitude (in decimal degrees): 41.26367°N	Longitude: 112.47527°W	
Datum: 		
Elevation: 1611m 	Map used: GPS		
General boulder shape (include in sketch): 		
Boulder/rock measurements: x-axis: 215 cm	y-axis: 247cm 	z-axis: 120cm  (above surface)	
Other pertinent length (specify) 			
Sketch rock (if desired): 			

After Collection: 	
Sample Thickness  32cm	Estimated Mass 	
Sample Length   3cm	Sample Width  23cm	
Azimuth 	Elevation Angle 		
340°	4°		
005°	2°		
015°	6°		
028°	8°		
030°	8°		
038°	15°		
048°	25°		
083°	15°		
130°	10°		
155°	0°